{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":23,"n_cols":4,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["USB - Microstecker"]
["Ministecker/Microstecker Pin ","Name ","Farbe ","Beschreibung"]
[1,"VCC ","Rot ","+5 V"]
[2,"D- ","Weiß ","Data -"]
[3,"D+ ","Grün ","Data +"]
[4,"ID ","keine ","erlaubt Unterscheidung von"]
[null,null,null,"Micro-A- und Micro-B-Stecker"]
[null,null,null,"Typ A: Masse"]
[null,null,null,"Typ B: nicht verbunden"]
[5,"GND ","Schwarz ","Masse"]
{"$rows_empty":12}
["Der Goldfisch braucht Typ A"]